**LOGIC GATES SIMULATOR SYSTEMS**

**A SEMINAR PAPER BY**

**IGBOEKWULUSI FRANKLIN CHINEDU**

**2017364022**

**DEPARTMENT OF ELECTRONIC AND COMPUTER ENGINEERING**

**NNAMDI AZIKIWE UNIVERSITY, AWKA**

**JANUARY 2023.**

**LOGIC GATES SIMULATOR SYSTEMS**

**A SEMINAR PAPER BY**

**IGBOEKWULUSI FRANKLIN CHINEDU**

**2017364022**

**IN PARTIAL FULFILMENT OF THE REQUIREMENTS FOR THE AWARD OF BACHELOR IN ENGINEERING (B.ENG)**

**DEPARTMENT OF ELECTRONIC AND COMPUTER ENGINEERING NNAMDI AZIKIWE UNIVERSITY, AWKA**

**JANUARY 2023.**

# **CERTIFICATION PAGE**

The seminar work “Logic gates Simulator Systems” was carried out by me under the supervision Engr. Dr. Kenneth Akpado and has not been submitted in part or full to this university or any other institutions for the award of a degree.

Igboekwulusi Franklin Chinedu Date

# 

# **APPROVAL PAGE**

This is to certify that this seminar paper written by ”Igboekwulusi Franklin Chinedu” with registration number 2017364022 has been supervised and approved by the Department of Electronics and Computer Engineering, Nnamdi Azikiwe University Awka by:

Engr. Dr. Kenneth Akpado Date

(Supervisor)

Engr. Dr. Kenneth Akpado Date

HOD, ECE Department

**DEDICATION**

I dedicate this report to the Almighty God for his faithfulness and grace upon my life and my family for their maximum support in my academic pursuits.

**ACKNOWLEDGEMENT**

My profound gratitude goes to God almighty and my wonderful parents for always being there for me.

My special thanks go to my supervisor Engr. Dr. Akpado K. A., Engr. Okechukwu G. N. and Ezeome A. B. for their firm guidance.

Heartfelt gratitude goes to all my lecturers Engr. Prof. Idigo Victor Eze, Engr. Prof. Okezie Christiana Chikodi, Engr. Prof. Azubogu Chukwuemeka Okwudili, Engr. Prof. Cletus Ogbonna Ohaneme, Engr. Dr. Akpado Keneth Aghaegbunam, Engr. Dr. Nnebe Scholastica Ukamaka, Engr. Dr. Okorogu Victor Ndubuisi, Engr. Dr. Ezeagwu Christtopher Ogwugwuam, Engr. Dr. Isizoh Anthony Nosike, Engr. Dr. Ufoaroh Stephen Uchenna, Engr. Dr. Alumona Theophilus Leonard, Engr. Dr. Obiora Dimson Ifeyinwa, Engr. Dr. Aniedu Azubuike Nzube, Engr. Dr. Oguejiofor Obinna Samuel, Engr. Dr. Udenze Adrain Igwebuike, Engr. Dr. Ogbodo Emmanuel Utochukwu, Engr. Nwalozie Gerald Chetachi, Engr. Dr. Onyeyili Innocent Tochukwu, Engr. Dr. Okafor Sunday Chukwuenye, Engr. Agodike Obinna Chidiebere, Engr. Dr. Alagbu Ekene Emmanuel, Ebih Uchenna Joseph. Ekwunife ThankGod Dozie, Obioma Peace Chibueze, Engr. Onuzulike Vincent Chukwuma, Engr. David Idakwo Friday, Nworabude Ekene Franklin; the graduate assistants Mr. Onubogu John Okechukwu, Eze Chikwado Emmanuel, Mbonu Chinedu Anthony; the chief technologists Engr. Okafor, Tyndale Chukwudi, Engr. Ejiofor, Herbert Chukwuemeka; assistant chief technologists Engr. Oguejiofor, John Uzochukwu,Ogu Chiedozie Darlington,Engr. Okechukwu Godson Nnaeto, and all other technologists and non-academic who have in one way or the other contributed to my academic pursuit so far.

And to my relatives and loved ones whose prayers, love and support towards my successful academic pursuit kept me going, I am really grateful.

**ABSTRACT**

Logic gate simulator systems are computer programs that allow users to design and simulate digital logic circuits. These systems provide a graphical user interface (GUI) for designing and simulating logic circuits, allowing users to create, edit, and debug their designs. The GUI typically includes a library of logic gates, such as AND, OR, NOT, NAND, NOR, XOR, and XNOR gates. Users can also add custom components to the library. The simulator then simulates the circuit's behavior in real-time and provides visual feedback on the circuit's operation. This allows users to quickly identify errors in their designs and make corrections before committing them to hardware. Logic gate simulator systems are used by engineers in the design of digital logic circuits for embedded systems and other applications.

**Table of content Page**

Title page ii

Certification page iii

Approval page iv

Dedication v

Acknowledgement vi

Abstract vii

Table of content viii

List of figures x

SECTION ONE: INTRODUCTION 1

1.1 Background of study 1

1.2 Brief history of logic gates simulators 2

SECTION TWO: DESIGN, FEATURES, TYPES AND EXAMPLES OF LOGIC GATE SIMULATOR SYSTEMS 3

2.1 Design of logic gate simulators systems 3

2.2 Features of logic gate simulator systems 4

2.3 Types of logic gate simulator systems 5

2.3.1 Operations performed by logic gate simulator systems 5

2.4 Examples of logic gate simulator systems 11

SECTION THREE: IMPORTANCE, USE, APPLICATIONS, ADVANTAGES AND DISADVANTAGES OF LOGIC GATE SIMULATOR SYSTEMS 14

3.1 Importance of logic gate simulator systems 14

3.2 Use of logic gate simulator systems 16

3.3 Applications of logic gate simulator systems 17

3.3 Advantages of logic gate simulator systems 18

3.4 Disadvantages of logic gate simulator systems 18

SECTION FOUR: CONCLUSION 19

REFRENCES 21

**LIST OF FIGURES**

Figure1: Diagram showing a design of a logic gate simulator system. Page 4

Figure 2: AND logic gate symbol Page 6

Figure 3: AND logic gate Truth table Page 6

Figure 4: AND logic gate symbol Page 6

Figure 5: AND logic gate Truth table Page 6

Figure 6: NOT logic gate symbol Page 7

Figure 7: NOT logic gate Truth table Page 7

Figure 8: NAND logic gate symbol Page 8

Figure 9: NAND logic gate Truth table Page 8

Figure 10: NOR logic gate symbol Page 8

Figure 11: NOR logic gate Truth table Page 8

Figure 12: XOR logic gate symbol Page 10

Figure 13: XOR logic gate Truth table Page 10

Figure 14: XNOR logic gate symbol Page 11

Figure 15: XNOR logic gate Truth table Page 11

Figure 16: Screen shot of Logisim 2.7.0 Page 12

Figure 17: Screen shot of CircuitVerse Page 13

Figure 18: Screen shot of Logicly 1.13.0 Page 14

Figure 19: Screen shot of Falstad Circuit Simulator Page 15

**SECTION ONE: INTRODUCTION**

* 1. **Background** **of** **study**

Logic Gate Simulator is an open-source tool for experimenting with and learning about logic gates. The simulator tool was originally designed for CIS students at [South Puget Sound Community College](http://www.spscc.ctc.edu/) but is free for anyone to use and modify under the GPL(General Public License) v3. Logic Gate Simulator is written in C#/WPF using .NET 4 [1]

Logic gate simulator systems are computer programs that allow users to simulate the behavior of logic gates. They are used to design and test digital circuits, and can be used to teach basic logic concepts. Logic gate simulators typically provide a graphical user interface (GUI) that allows users to create and manipulate logic gates, as well as simulate their behavior. The GUI usually includes a library of logic gates, which can be dragged and dropped onto the workspace. The user can then connect the gates together to form a circuit, and then run simulations to see how the circuit behaves under different input conditions.

* + 1. **Brief History of Logic Gate Simulators**  
       Logic gate simulators have been around since the early days of computing. The first logic gate simulator was developed in the 1950s by IBM for use in their computers. This simulator was used to test and debug logic circuits before they were implemented in hardware.

In the 1970s, the first commercial logic gate simulators were released. These simulators allowed users to design and simulate digital circuits on their personal computers. They also allowed users to create custom logic gates and simulate them in real-time.

Since then, many different types of logic gate simulators have been developed, including those for educational purposes, professional engineering applications, and even gaming applications. Today, there are a variety of free and commercial logic gate simulators available for use on both desktop and mobile devices.[2]

**SECTION TWO: DESIGN, TYPES AND EXAMPLES OF LOGIC GATE SIMULATOR SYSTEMS**

**2.1 Design of a logic gate simulator**  
A logic gate simulator is a computer program that allows users to simulate the behavior of logic gates. It is designed to help students and engineers understand how logic gates work and how they can be used in digital circuits.

The design of a logic gate simulator should include a graphical user interface (GUI) that allows users to easily create and manipulate logic gates. The GUI should also provide an easy way for users to connect the inputs and outputs of the logic gates.

The GUI should also provide an easy way for users to view the output of the circuit as it changes with different inputs.

The simulator should also include a library of pre-defined logic gates, such as AND, OR, NOT, NAND, NOR, XOR, etc., so that users can quickly create complex circuits without having to manually define each gate. The library should also include more advanced gates such as flip-flops and multiplexers.

The simulator should also include a simulation engine that can accurately simulate the behavior of the circuit based on its inputs and outputs. This engine should be able to accurately simulate both digital and analog signals so that users can accurately test their designs before building them in real life.

Finally, the simulator should include debugging tools so that users can easily identify any errors in their designs or simulations. These tools could include breakpoints, watchpoints, trace points, etc., which allow users to pause or step through their simulations in order to identify any issues with their designs or simulations.




Figure 1 diagram showing a design of a logic gate simulator system.

**2.2 Features of logic gate simulator systems**

Logic gate simulator systems has the following features:

1. **Visual Representation:** Logic gate simulators provide a visual representation of the logic gates and their connections, allowing users to easily understand the circuit design.
2. **Simulation:** Logic gate simulators allow users to simulate the behavior of a circuit by providing inputs and observing the outputs. This allows users to test their designs before committing to hardware implementation.
3. **Debugging:** Logic gate simulators provide debugging features that allow users to identify errors in their designs and make corrections before committing to hardware implementation.

A variety of debugging tools that can be used to identify errors in circuits or debug simulations, such as breakpoints, watchpoints, and trace points that allow users to step through simulations one instruction at a time and observe what is happening at each step along the way.

1. **Timing Analysis:** Logic gate simulators can be used to analyze the timing of a circuit, allowing users to optimize their designs for speed or power consumption.
2. **Library of components:** Most logic gate simulators come with a library of components that can be used in designing circuits, such as logic gates, flip-flops, multiplexers, etc.
3. **Scripting Language Support:** The ability to write scripts in a supported language (such as Python) that can be used to automate certain tasks within the simulator environment, such as setting up simulations or running tests on circuits automatically without user intervention.
4. **Logic Analyzer:** The ability to monitor and analyze logic signals in real-time or after a simulation has completed.
5. **Waveform Viewer:** The ability to view waveforms of logic signals in real-time or after a simulation has completed.
6. **Simulation Speed:** The ability to adjust the speed of the simulation, allowing for faster or slower simulations as needed.

**2.3 Types of logic gate simulator systems**

We have 3 basic types of logic gate simulator systems which includes:

1. **Digital Logic Gate Simulator**: A digital logic gate simulator is a software program that allows users to design and simulate digital logic circuits. It typically includes a library of logic gates, such as AND, OR, NOT, NAND, NOR, XOR and XNOR gates. The user can then connect these gates together to create more complex circuits.

**2.3.1 Operations performed by digital logic gate simulator systems**

**i. AND operation using a logic gate simulator**

The Logic AND Gate is a type of digital logic circuit whose output goes HIGH to a logic level 1 only when all of its inputs are HIGH

The output state of a digital logic AND gate only returns “LOW” again when ANY of its inputs are at a logic level “0”. In other words for a logic AND gate, any LOW input will give a LOW output.

The logic or Boolean expression given for a digital AND gate is that for Logical Multiplication which is denoted by a single dot or full stop symbol, ( . ) giving us the Boolean expression of: A.B = Q.

Then we can define the operation of a digital 2-input AND gate as being:



“If both A and B are true, then Q is true”[3]

Figure 2: AND logic gate symbol Figure 3: AND logic gate Truth table

1. **OR operation using a logic gate simulator**

The Logic OR Gate is a type of digital logic circuit whose output goes HIGH to a logic level 1 only when one or more of its inputs are HIGH

The output, Q of a “Logic OR Gate” only returns “LOW” again when ALL of its inputs are at a logic level “0”. In other words for a logic OR gate, any “HIGH” input will give a “HIGH”, logic level “1” output.

The logic or Boolean expression given for a digital logic OR gate is that for Logical Addition which is denoted by a plus sign, ( + ) giving us the Boolean expression of: A+B = Q.

Thus the OR gate can be correctly described as an “Inclusive OR gate” because the output is true when both of its inputs are true (HIGH). Then we can define the operation of a 2-input logic OR gate as being:


“If either A or B is true, then Q is true”[4]

Figure 4: AND logic gate symbol Figure 5: AND logic gate Truth table

1. **NOT operation using a logic gate simulator**

The Logic NOT Gate is the most basic of all the logical gates and is often referred to as an Inverting Buffer or simply an Inverter.

Inverting NOT gates are single input devise which have an output level that is normally at logic level “1” and goes “LOW” to a logic level “0” when its single input is at logic level “1”, in other words it “inverts” (complements) its input signal. The output from a NOT gate only returns “HIGH” again when its input is at logic level “0” giving us the Boolean expression of: A = Q.

Then we can define the operation of a single input digital logic NOT gate as being:

“If A is NOT true, then Q is true”[5]




Figure 6: NOT logic gate symbol Figure 7: NOT logic gate Truth table


1. **NAND operation using a logic gate simulator**

The Logic NAND Gate is a combination of a digital logic AND gate and a NOT gate connected together in series.

The NAND (Not – AND) gate has an output that is normally at logic level “1” and only goes “LOW” to logic level “0” when ALL of its inputs are at logic level “1”. The Logic NAND Gate is the reverse or “Complementary” form of the AND gate.

The logic or Boolean expression given for a logic NAND gate is that for Logical Addition, which is the opposite to the AND gate, and which it performs on the complements of the inputs. Its Boolean expression is denoted by a single dot or full stop symbol, ( . ) with a line or Overline, ( ‾‾ ) over the expression to signify the NOT or logical negation of the NAND gate giving us the Boolean expression of: A.B = Q.

Then we can define the operation of a 2-input digital device as being:

“If both A and B are true, then Q is NOT true”[6]




Figure 8: NAND logic gate symbol Figure 9: NAND logic gate Truth table


1. **NOR operation using a logic gate simulator**

The Logic NOR Gate is a combination of the digital logic OR gate and an inverter or NOT gate connected together in series.

The inclusive NOR (Not-OR) gate has an output that is normally at logic level “1” and only goes “LOW” to logic level “0” when ANY of its inputs are at logic level “1”. The Logic NOR Gate is the reverse or “Complementary” form of the inclusive OR gate.

The logic or Boolean expression given for a logic NOR gate is that for Logical Multiplication which it performs on the complements of the inputs. Its Boolean expression is denoted by a plus sign, ( + ) with a line or Overline, ( ‾‾ ) over the expression to signify the NOT or logical negation of the NOR gate giving us the Boolean expression of: A+B = Q.

Then we can define the operation of a 2-input digital gate as being:

“If both A and B are NOT true, then Q is true”[7]




Figure 10: NOR logic gate symbol Figure 11: NOR logic gate Truth table

1. **XOR operation using a logic gate simulator**

The Exclusive-OR logic function is a very useful circuit that can be used in many different types of computational circuits.

The “Exclusive OR Gate” is another type of digital logic gate commonly used in arithmetic operations since it can be used to give the sum of two binary numbers as well as error-detection and correction circuits.

In the previous tutorials, we saw that by using the three principal gates, the AND Gate, the OR Gate and the NOT Gate, we can build many other types of logic gate functions, such as a NAND Gate and a NOR Gate or any other type of digital logic function we can imagine.

But there are two other types of digital logic gates which although they are not a basic gate in their own right as they are constructed by combining together other logic gates, their output Boolean function is important enough to be considered as complete logic gates. These two “hybrid” logic gates are called the Exclusive-OR (Ex-OR) Gate and its complement the Exclusive-NOR (Ex-NOR) Gate.

Previously, we saw that for a 2-input OR gate, if A = “1”, OR B = “1”, OR BOTH A + B = “1” then the output from the digital gate must also be at a logic level “1” and because of this, this type of logic gate is known as an Inclusive-OR function. The logic gate gets its name from the fact that it includes the case of Q = “1” when both A and B = “1”.

If however, an logic output “1” is obtained when ONLY A = “1” or when ONLY B = “1” but NOT both together at the same time, giving the binary inputs of “01” or “10”, then the output will be “1”. This type of gate is known as an Exclusive-OR function or more commonly an Ex-Or function for short. This is because its boolean expression excludes the “OR BOTH” case of Q = “1” when both A and B = “1”.

In other words the output of an Exclusive-OR gate ONLY goes “HIGH” when its two input terminals are at “DIFFERENT” logic levels with respect to each other.

An odd number of logic “1’s” on its inputs gives a logic “1” at the output. These two inputs can be at logic level “1” or at logic level “0” giving us the Boolean expression of: Q = (A ⊕ B) = A.B + A.B

The Exclusive-OR Gate function, or Ex-OR for short, is achieved by combining standard logic gates together to form more complex gate functions that are used extensively in building arithmetic logic circuits, computational logic comparators and error detection circuits.



The two-input “Exclusive-OR” gate is basically a modulo two adder, since it gives the sum of two binary numbers and as a result are more complex in design than other basic types of logic gate.[8]

Figure 12: XOR logic gate symbol Figure 13: XOR logic gate Truth table 

1. **XNOR operation using a logic gate simulator**

The Exclusive-NOR Gate function is a digital logic gate that is the reverse or complementary form of the Exclusive-OR function.

Basically the “Exclusive-NOR Gate” is a combination of the Exclusive-OR gate and the NOT gate but has a truth table similar to the standard NOR gate in that it has an output that is normally at logic level “1” and goes “LOW” to logic level “0” when ANY of its inputs are at logic level “1”.

However, an output “1” is only obtained if BOTH of its inputs are at the same logic level, either binary “1” or “0”. For example, “00” or “11”. This input combination would then give us the Boolean expression of: Q = (A ⊕ B) = A.B + A.B

Then the output of a digital logic Exclusive-NOR gate ONLY goes “HIGH” when its two input terminals, A and B are at the “SAME” logic level which can be either at a logic level “1” or at a logic level “0”. In other words, an even number of logic “1’s” on its inputs gives a logic “1” at the output, otherwise is at logic level “0”.

Then this type of gate gives and output “1” when its inputs are “logically equal” or “equivalent” to each other, which is why an Exclusive-NOR gate is sometimes called an Equivalence Gate.

The logic symbol for an Exclusive-NOR gate is simply an Exclusive-OR gate with a circle or “inversion bubble”, ( ο ) at its output to represent the NOT function. Then the Logic Exclusive-NOR Gate is the reverse or “Complementary” form of the Exclusive-OR gate, (A ⊕ B).[9]





Figure 14: XNOR logic gate symbol Figure 15: XNOR logic gate Truth table

1. **Analog Logic Gate Simulator**: An analog logic gate simulator is a software program that allows users to design and simulate analog logic circuits. It typically includes a library of analog components such as resistors, capacitors and transistors. The user can then connect these components together to create more complex circuits.
2. **Programmable Logic Gate Simulator**: A programmable logic gate simulator is a software program that allows users to design and simulate programmable logic circuits. It typically includes a library of programmable logic devices such as FPGAs (Field Programmable Gate Arrays) and CPLDs (Complex Programmable Logic Devices). The user can then connect these devices together to create more complex circuits.

**2.4 Examples of logic gate simulator systems**

Here are 4 examples of logic gate simulator systems which includes:

1. **Logisim:** Thisis an educational tool for designing and simulating digital logic circuits. With its simple toolbar interface and simulation of circuits as you build them, it is simple enough to facilitate learning the most basic concepts related to logic circuits**.**

The logisim simulator software has the following features:

* It is free! (Logisim is open-source ([GPL](http://www.cburch.com/logisim/gpl.html)).)
* It runs on any machine supporting Java 5 or later; special versions are released for MacOS X and Windows. The cross-platform nature is important for students who have a variety of home/dorm computer systems.
* The drawing interface is based on an intuitive toolbar. Color-coded wires aid in simulating and debugging a circuit.
* The wiring tool draws horizontal and vertical wires, automatically connecting to components and to other wires. It's very easy to draw circuits!
* Completed circuits can be saved into a file, exported to a GIF file, or printed on a printer.
* Circuit layouts can be used as "subcircuits" of other circuits, allowing for hierarchical circuit design.
* Included circuit components include inputs and outputs, gates, multiplexers, arithmetic circuits, flip-flops, and RAM memory.
* The included "combinational analysis" module allows for conversion between circuits, truth tables, and Boolean expressions.[10]




Figure 16 Screen shot of Logisim 2.7.0

1. **CircuitVerse:** CircuitVerse is an online logic gate simulator system that allows users to design, simulate, and share their own digital circuits. It features a modern web-based interface with drag-and-drop components, and supports both combinational and sequential logic.

The circuit verse simulator software has the following features

* **Export High-Resolution Images:** CircuitVerse can export high-resolution images in multiple formats including SVG.
* **Combinational Analysis:** Automatically generate circuit based on truth table data. This is great to create complex logic circuits and can be easily be made into a subcircuit.
* **Embed in Blogs:** Since CircuitVerse is built in HTML5, an iFrame can be generated for each project allowing the user to embed it almost anywhere.
* **Use Sub circuits:** Create subcircuits once and use them repeatedly. This allows easier and more structured design.
* **Multi Bit Buses and components:** CircuitVerse supports multi bit-wires, this means circuit design is easier, faster, and uncluttered.





Figure 17 Screen shot of CircuitVerse

1. **Logicly:** Logicly is a paid logic gate simulator system that allows users to design, simulate, and debug digital circuits. It features an intuitive graphical user interface with drag-and-drop components, and supports both combinational and sequential logic.

The circuit verse simulator software has the following features

* **Logic gates:** Includes all of the standard gates you need — such as AND, OR, NOT, XOR, NAND, NOR, and XNOR. Includes many other primitives, including tri-state buffers and pull up/down resistors.
* **Truth tables:** Analyze all parts of your circuit with automatically generated truth tables. You can create a table for the current selection, for a custom integrated circuit, or even for your entire file. You can export the table as a CSV file too.
* **Simulation controls:** Pause the simulation, and step through it to watch how the signal propagates. Or, reset the simulation entirely to start fresh in a "just turned on" state.
* **Logic signal types:** The simulation supports four types of signals, including true (1), false (0), high impedence (hi-z) and a special error state. Any of these signals may be used as the default for inputs too.
* **Import/export circuit libraries:** Customize Logicly for your curriculum by building libraries of custom circuits that students can "import" into their work.

Figure 18 Screen shot of Logicly 1.13.0

1. **Falstad Circuit Simulator:** Falstad Circuit Simulator is a free online logic gate simulator system that allows users to design, simulate, and share their own digital circuits. It features an intuitive graphical user interface with drag-and-drop components, and supports both combinational and sequential logic.

The circuit verse simulator software has the following features

* Fixed import/export when running as an applet
* Ability to save/load to/from a file when running as an application
* The circuits that appear in the "Circuit" menu may now be bundled with the jar file.
* WireElm is now a subclass of ResistorElm (without this change, whenever you use two switches in parallel, you get the error "voltage source/wire loop with no resistance").[12]




Figure 19 Screen shot of Falstad Circuit Simulator

**SECTION THREE: IMPORTANCE, USES APPLICATIONS, ADVANTAGES AND DISADVANTAGES OF LOGIC GATE SIMULATOR SYSTEMS.**

**3.1 Importance of logic gate simulator systems.**

Logic gate simulator systems are important for a variety of reasons.

1. They allow engineers and students to design, test, and debug digital circuits without the need for physical components.
2. They also save time and money in the development process, as well as reduce the risk of errors due to incorrect wiring or component selection.
3. They also give a visual representation and behavior of a circuit before it’s been implemented using the real items.
4. They also have a variety of components in their library which gives an engineer multiple options to choose from while designing a circuit.
5. Finally, it also has a good feedback system which tells the engineer if the component used in designing a circuit is actually compactible with the system.
   1. **Uses of logic gate simulator systems.**

Logic gate simulator systems is used and is applied in different areas

1. Logic gate simulators are used to teach students the fundamentals of digital logic and computer engineering. By providing a virtual environment for students to explore and experiment with, they can gain a better understanding of the principles behind digital logic and computer engineering.
2. Logic gate simulators are used to develop and test new designs for digital circuits. By providing a virtual environment for engineers to design, simulate, and debug their designs, they can quickly identify any potential problems before committing to physical implementation.
3. Logic gate simulators are used in the development of embedded systems such as microcontrollers and FPGAs (Field Programmable Gate Arrays). By providing a virtual environment for engineers to design, simulate, and debug their designs, they can quickly identify any potential problems before committing to physical implementation.
4. Logic gate simulators are also useful tools for troubleshooting existing digital circuits. By using simulation software, engineers can analyze existing circuits without having access them physically. This allows them diagnose issues more efficiently without having access them physically.
5. Logic gate simulators are used in the development of communication networks such as cellular networks or Wi-Fi networks. By providing a virtual environment for engineers to design, simulate, and debug their designs, they can quickly identify any potential problems before committing to physical implementation.
6. Logic gate simulators are used in the development of aerospace systems such as aircraft navigation systems or satellite communication networks. By providing a virtual environment for engineers to design, simulate, and debug their designs, they can quickly identify any potential problems before committing to physical implementation.
7. Finally, these systems can be used to simulate complex systems that would otherwise be too expensive or difficult to build in the real world.
   1. **Applications of logic gate simulator systems**

Logic gate simulator systems are applied in the development of: [4]

1. NAND Gates which are used in Burglar alarms and buzzers.
2. Push buttons which are used in the creation of switches.
3. AND Gates which are used to enable the data transfer function.
4. TTL (Transistor Transistor Logic) and CMOS circuitry.
5. Circuits which involves computation and processing.
6. Embedded system designs
7. Robotics control system
   1. **Advantages of logic gate simulator systems**

Logic gate simulator systems has various advantages: [5]

1. **Building Blocks**: They are the building blocks of any digital device, so in a nutshell digital devices won’t work perfectly without being well simulated.
2. **Faster:** Logic gate simulator systems are faster when it comes to solving any complex problems.
3. **Cheap:**Logic gate simulator systems are mostly cheap if they are to be purchased and also have free ones.
4. **Requires less power:**Logic gate simulator systems do not require much power for it’s operation.
   1. **Disadvantages of logic gate simulator systems**

Logic gate simulator systems has some disadvantages which some of them are:

1. **Limited Capabilities:** Logic gate simulators are limited in their capabilities and may not be able to accurately simulate complex logic circuits.
2. **Cost:** Logic gate simulators can be expensive, especially for more advanced versions.
3. **Time-Consuming:** Simulating a logic circuit can be time-consuming, as the user must manually enter each component and its associated parameters into the simulator.
4. **Difficulty to use:** Logic gate simulators can be difficult to use, especially for those who are unfamiliar with the software or the underlying concepts of digital logic design.

**SECTION FOUR: CONCLUSION**

Logic gate simulator systems are an important tool for engineers and scientists to design, test, and debug digital circuits. They allow users to simulate the behavior of a circuit before it is built, saving time and money. This seminar focused on the various types and examples of logic gate simulators available, their features, and how they can be used in a variety of applications.

The first part of the seminar discussed the design, features, examples and types of logic gate simulators available. In which some of it’s features includes support for multiple logic gates, timing analysis tools, debugging capabilities, simulation speed, logic analyzer, scripting language support, debugging tools and more. It is important to understand these features in order to make an informed decision when selecting a simulator for a particular application.

Some examples of the software-based simulators are Logisim, Logicly, Falstad Circuit Simulator and CircuitVerse. Each one has its own advantages and disadvantages, so it is important to choose the right one for the application at hand.

We also discussed the 3 main types of logic gate simulator systems which include digital logic gate simulator, analog logic gate simulator and programmable logic gate simulators, which we focused on the digital logic gate simulator systems which includes:

* AND Gate and its mode of operation in a logic gate simulator system
* OR Gate and its mode of operation in a logic gate simulator system
* NOT Gate and its mode of operation in a logic gate simulator system
* XOR Gate and its mode of operation in a logic gate simulator system
* XNOR Gate and its mode of operation in a logic gate simulator system
* NAND Gate and its mode of operation in a logic gate simulator system
* NOR Gate and its mode of operation in a logic gate simulator system

The second part of the seminar discussed how logic gate simulators can be used in various applications, it’s importance, it’s advantages and disadvantages. Most of it’s applications include digital signal processing (DSP), embedded systems design, robotics control systems, and more. It is important to understand how each application works in order to select the right simulator for it.

Although in modern day systems and devices, micro-controllers and micro-processors are applied for both the design and it’s circuit implementation. But these micro- processors and micro-controllers contains logic gates embedded in them and for us to monitor the behavior and output of these circuits before the actual circuit implementation, we would have to use a logic gate simulator system to do that.

Overall, this seminar provided an overview of logic gate simulator systems and their uses in various applications. It highlighted their advantages over traditional methods of circuit design and debugging while also providing best practices for successful implementation.

References:

[1] Steve Kollmansberger, “- Logic Gates Simulator” in *kolls.net/gatesim,* united states, 2009.

[2] Frank AI, in *frankai.netlify.app,* Nigeria,2022.

[3] W. Storr, “Logic and gate tutorial with the logic and gate truth table,” *Basic Electronics Tutorials*, 05-Aug-2022. [Online]. Available: https://www.electronics-tutorials.ws/logic/logic\_2.html. [Accessed: 17-Jan-2023].

[4] “Or gate,” Wikiwand. [Online]. Available: https://www.wikiwand.com/en/OR\_gate. [Accessed: 17-Jan-2023].

[5] W. Storr, “Logic not gate tutorial with Logic Not Gate Truth table,” *Basic Electronics Tutorials*, 05-Aug-2022. [Online]. Available: https://www.electronics-tutorials.ws/logic/logic\_4.html. [Accessed: 17-Jan-2023].

[6] W. Storr, “Logic NAND gate tutorial with logic NAND gate truth table,” *Basic Electronics Tutorials*, 05-Aug-2022. [Online]. Available: https://www.electronics-tutorials.ws/logic/logic\_5.html. [Accessed: 17-Jan-2023].

[7] W. Storr, “Logic nor gate tutorial with Logic Nor Gate Truth table,” *Basic Electronics Tutorials,* 05-Aug-2022. [Online]. Available: https://www.electronics-tutorials.ws/logic/logic\_6.html. [Accessed: 17-Jan-2023].

[8] W. Storr, “Exclusive-or gate tutorial with ex-OR gate truth table*,” Basic Electronics Tutorials*, 05-Aug-2022. [Online]. Available: https://www.electronics-tutorials.ws/logic/logic\_7.html. [Accessed: 17-Jan-2023].

[9] W. Storr, “Exclusive-nor gate tutorial with ex-NOR gate truth table,” *Basic Electronics Tutorials*, 05-Aug-2022. [Online]. Available: https://www.electronics-tutorials.ws/logic/logic\_8.html. [Accessed: 17-Jan-2023].

[10] Logisim. [Online]. Available: http://www.cburch.com/logisim/. [Accessed: 17-Jan-2023].

[11] “Logic.ly features*,” Features - Logicly Documentation.* [Online]. Available: https://logic.ly/features/. [Accessed: 17-Jan-2023].

[12] Hausen, “Hausen/circuit-simulator: Paul Falstad's circuit simulator (with improvements),” GitHub. [Online]. Available: https://github.com/hausen/circuit-simulator. [Accessed: 17-Jan-2023].

[13] L. Ashrit, “*Logic gates - types, working principle, application, advantage,”* electricalfundablog.com, 07-Nov-2019. [Online]. Available: https://electricalfundablog.com/logic-gates-types-working-principle/. [Accessed: 17-Jan-2023].

[14] Sanchit Jain, “*What is the advantage of Logic Gate?,*” Quora. [Online]. Available: https://www.quora.com/What-is-the-advantage-of-logic-gate. [Accessed: 17-Jan-2023].